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WATERBLOK RUBBERISED BITUMEN

EMULSION WATERPROOFING

COMPOUND

DESCRIPTION

WATERBLOK Rubberised Waterproofing Compound (R.W.P.C.).is a mineral filled emulsion of a refined grade of bitumen which contains a high percentage of rubber latex.  It is a multi-purpose waterproofing and sealing compound.  It is a water based emulsion and requires no heating. The product has the consistency of a soft paste and is thixotropic. It is thus very easy to apply with brushes or soft brooms.

TYPICAL USES
WATERBLOK R.W.P.C.after drying gives a highly elastic bituminous film which is impervious to water.  It is an excellent sealing compound for walls, parapet walls, flashings, roofs, reservoirs and fish ponds etc.  It  may be applied to asphalt, asbestos cement, concrete, corrugated iron, lead, zinc, roofing felt and similar surfaces whether flat, sloping, or vertical.  It can be used on its own when applied to sound surfaces that are free of cracks and joints, or in conjunction with geotextile fabric where there is any possibility of movement in cracks or joints.

SPECIAL CHARACTERISTICS
A high percentage of rubber latex imparts considerable elasticity to the dried film.

PREPARATION

Remove all dust, dirt and rust.  Where moss and lichen etc are present, this should be removed, and the surface treated with fungicide which should be allowed to dry before the WATERBLOK treatment proceeds. Stir contents of tin before use.

APPLICATION

1) WATERBLOK can be applied to both damp (and drying), and dry surfaces with soft brushes or brooms which should be dampened with water before, and occasionally during use, to avoid clogging  and to ensure ease of application.  To promote adhesion and spreading in very hot weather and on absorbent surfaces, dampen the surface with water.

2) Porous surfaces such as brickwork, concrete or asbestos-cement should first be primed with a coat of WATERBLOK R.W.P.C. diluted 50/50 with water. Allow to dry before proceeding.

3) WATERBLOK R.W.P.C. is brushed on but is not a paint. It is a waterproofing coating and should be applied at a thickness of approximately 1mm for best results. Recommended coverage is therefore 1litre per m2 per layer to achieve desired film thickness.

4) A second application is recommended to waterproof porous surfaces and to provide a thoroughly durable covering. Each coat must be dry before the next is applied. Drying time will be approximately 2 - 3 hours in sunny weather.

5) Where joints,cracked or unstable areas need to be treated, it is advisable to embed non-woven polyester geofabric membrane into the first full strength coat of WATERBLOK immediately after application while the product is still wet. After drying, a further two coats should be applied over the membrane.  This system creates a very effective and flexible waterproof membrane. In cases where the product is used together with membrane the total application for all coats is approximately 3 litres per sq.m (excluding the prime coat).

6) When waterproofing cement dams or ponds, particularly where they are excavated below ground level, care should be taken to ensure that no free moisture is migrating through the wall and inhibiting the drying of the product.  The surrounding ground should be dry and there should be no signs of dampness or moisture inside the pond.  After applying the product, ensure that it is properly cured and dry before proceeding with following applications. There should be no wet, brown areas visible once the product has cured correctly.  The use of membrane is recommended in area's which are very porous, or where cracks or joints are present.

NOTE:

a)   Do not apply if rain appears probable within a few hours. Ideally WATERBLOK should be applied during the morning of a sunny day. To test for proper curing, rub the surface with a wet finger. Once dry, WATERBLOK R.W.P.C. will not cause brown staining.

b)  WATERBLOK R.W.P.C. should not be applied to surfaces previously treated with tar-based materials unless such materials have weathered for two to three years.

c)  Brushes or brooms should be washed in clean water immediately after use; if clogged, they can be cleaned with paraffin or white spirit. These solvents should not be used on brushes or brooms during application.

SPECIFICATION

Product Type
 

:
Bitumen emulsion containing rubber latex

Product Consistency

:
Soft thixotropic paste.

Colour



:         
Black when dry.

Drying time:   
 

:         
2-3 hours outdoors on a sunny day.

Water Permeability

:       
Impervious to depths of 5m     

Flash Point:     

:       
Non inflammable

Fire Resistance

:       
Low fire spread

Mass per litre


:      
1.05 kilograms

Availability


:         
1 litre, 5 litre, 20 litre, 200 litre containers

Effect of U.V. 


:
Viaseal Waterblok film has withstood 500 hrs in SABS 




weatherometer.    SABS 1134-77

Toxicity to water

: 
None. SABS 1217

Elong.@ B. Point  

:  
100%  SABS 952 - 1969

Acid Resistance

:
Unaffected by 30% sulphuric acid. (1 year @
 




25oC).
Softening point

:
91oC

Ductility @ 10oC

:
> 100 cm
Elastic Recovery @ 10oC
:
47.5%

Solids Content


:
61%
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